**General Info**

username: pi

password: Aa123456

Network name: PiNetwork

Network password: ESC204LMR

**SSH to Pi**

1. connect power supply to pi
2. wait approx 75 seconds for pi to boot up
3. go to wifi connections on your device, connect to **PiNetwork**
4. enter password **ESC204LMR**
5. On windows: using putty, connect to ip address: **192.168.4.1**
6. enter username: **pi**
7. enter password: **Aa123456**
8. you are now in the /pi/home folder

For reference about SSH: <https://www.raspberrypi.org/documentation/configuration/wireless/access-point.md>

**VNC into Pi (requires monitor and keyboard)**

1. connect pi to power supply, mouse, keyboard, monitor